Activity – 24358 (v2) Plan and monitor the construction of a BCATS project and quality check the product

Student name:

Once the job specifications have been received and confirmed, what should we look for when checking them in detail before commencing the production of the job?

Why is it important to maintain a clean and efficient working environment?

The top of a saw stool has to be cut to a length of 700 mm +/- 10mm. What range of sizes would be acceptable to meet the requirements of the job specifications?

Identify the range of sizes that would be deemed acceptable for the following specifications within tolerances as specified.

500mm (with a tolerance of -5mm):

720mm x 265mm (with a tolerance of +/- 5mm):

What information is contained in the specifications?

What must be done if a person is unsure of any part of a job specification?

Why is it necessary to implement quality checks at each stage of the job?

List 4 quality control methods that could be used during the construction of a project.

1. 2. 3. 4.