Learner Self-reflection – 31860 (v1) Construct and maintain a basic residential timber fence as a BCATS project

Student name:

How deep should posts be set in the ground for a 1200mm high fence?

How many rails are recommended for fences above 1.2m and why?

What are 2 methods that can be used for installing rails to posts?

1. 2.

What size gap should you allow between the palings and the ground?

Why is it important to check a fence regularly for damage and wear?

What kind of metal protection is required for gate and fence hardware and fastenings?